1. Run setup.exe to install the Loader Program.
2. Switch off the Vicatronic.
3. Connect the Vicatronic to the Pc by a RS232 cable.
4. Run the Loader software.
5. Select from the File menu the following function: File->Open->Motorola S-Record.
6. Open from your documents the following file: Vicat  02.04.000 - Vicatronic.s19
7. Click on the button “Program”.
8. When the PC shows the message “wait for synchronization” switch on the Vicatronic.
9. The Loader Program will automatically send the new firmware.
10. At the end, switch off the Vicatronic and disconnect the serial cable.
